HPD 385 Measurements

30 dbfs input from REW

Measurement made with Fluke 289 in volts rms  , drivers connected to Pass F6 , common ground from DAC to driver .
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